;/*++
;
; Realtek Wireless 802.11b/g/n USB 2.0 Network Adapter Selective Suspend Enabler
; 
; Copyright (C) 2010 Realtek Semiconductor Corp.
;
; Module Name:
;
;    rtlss.INF
;
; Abstract:
;    INF for installing selective suspend enabler
;
;--*/

[Version]
Signature="$WINDOWS NT$"
Class=USB
ClassGUID={36fc9e60-c465-11cf-8056-444553540000} 
Provider=%MfgName%
CatalogFile.NT	= rtlss.cat		;; for WHQL certified
DriverVer=11/16/2010,6.1.7600.16385

; ================= Class section =====================

[ClassInstall32]
Addreg=USBClassReg     

[USBClassReg]
HKR,,,0,%ClassName%
HKR,,Icon,,-5

; ================= Device section =====================

[Manufacturer]
%MfgName%=Microsoft,NTx86

; For Win2K
[Microsoft]
%RTL8188SU.DeviceDesc%=rtlss.Dev, USB\VID_0BDA&PID_8171&REV_0200
%RTL8188SU.DeviceDesc%=rtlss.Dev, USB\VID_1690&PID_0752&REV_0200
%RTL8191SU.DeviceDesc%=rtlss.Dev, USB\VID_0BDA&PID_8172&REV_0200
%RTL8191SU.DeviceDesc%=rtlss.Dev, USB\VID_13D3&PID_3309
%RTL8191SU.DeviceDesc%=rtlss.Dev, USB\VID_13D3&PID_3339
%RTL8191SU.DeviceDesc%=rtlss.Dev, USB\VID_13D3&PID_3340
%RTL8191SU.DeviceDesc%=rtlss.Dev, USB\VID_13D3&PID_3341
%RTL8192GU.DeviceDesc%=rtlss.Dev, USB\VID_0BDA&PID_8173&REV_0200
%RTL8192SU.DeviceDesc%=rtlss.Dev, USB\VID_0BDA&PID_8174&REV_0200
; Add CU series UPDATE TO DID table V38
; 8188CUS
%RTL8188CU.DeviceDesc%=rtlss.Dev, USB\VID_0BDA&PID_8176&REV_0200
%RTL8188CU.DeviceDesc%=rtlss.Dev, USB\VID_0BDA&PID_8176
%RTL8188CU.DeviceDesc%=rtlss.Dev, USB\VID_0BDA&PID_8177&REV_0200
%RTL8188CU.DeviceDesc%=rtlss.Dev, USB\VID_0BDA&PID_8177
%RTL8188CU.DeviceDesc%=rtlss.Dev, USB\VID_2019&PID_ED17
%RTL8188CU.DeviceDesc%=rtlss.Dev, USB\VID_0DF6&PID_0052
%RTL8188CU.DeviceDesc%=rtlss.Dev, USB\VID_7392&PID_7811
%RTL8188CU.DeviceDesc%=rtlss.Dev, USB\VID_07B8&PID_8189
%RTL8188CU.DeviceDesc%=rtlss.Dev, USB\VID_0EB0&PID_9071
%RTL8188CU.DeviceDesc%=rtlss.Dev, USB\VID_06F8&PID_E033
%RTL8188CU.DeviceDesc%=rtlss.Dev, USB\VID_103C&PID_1629
%RTL8188CU.DeviceDesc%=rtlss.Dev, USB\VID_2001&PID_3308
%RTL8188CU.DeviceDesc%=rtlss.Dev, USB\VID_050D&PID_1102
%RTL8188CU.DeviceDesc%=rtlss.Dev, USB\VID_2019&PID_AB2A
%RTL8188CU.DeviceDesc%=rtlss.Dev, USB\VID_20F4&PID_648B
%RTL8188CU.DeviceDesc%=rtlss.Dev, USB\VID_4855&PID_0090
;8192 CU
%RTL8192CU.DeviceDesc%=rtlss.Dev, USB\VID_0BDA&PID_8178&REV_0200
%RTL8192CU.DeviceDesc%=rtlss.Dev, USB\VID_0BDA&PID_8178
%RTL8192CU.DeviceDesc%=rtlss.Dev, USB\VID_2001&PID_3307
%RTL8192CU.DeviceDesc%=rtlss.Dev, USB\VID_2001&PID_330A
%RTL8192CU.DeviceDesc%=rtlss.Dev, USB\VID_2001&PID_3309
%RTL8192CU.DeviceDesc%=rtlss.Dev, USB\VID_0586&PID_341F
%RTL8192CU.DeviceDesc%=rtlss.Dev, USB\VID_7392&PID_7822
%RTL8192CU.DeviceDesc%=rtlss.Dev, USB\VID_2019&PID_AB2B
%RTL8192CU.DeviceDesc%=rtlss.Dev, USB\VID_07B8&PID_8178
%RTL8192CU.DeviceDesc%=rtlss.Dev, USB\VID_07AA&PID_0056
%RTL8192CU.DeviceDesc%=rtlss.Dev, USB\VID_4855&PID_0091
;8188 RU
%RTL8188RU.DeviceDesc%=rtlss.Dev, USB\VID_0BDA&PID_817D&REV_0200
%RTL8188RU.DeviceDesc%=rtlss.Dev, USB\VID_0BDA&PID_817D
; 8188CE_VAU
%RTL8188CE_VAU.DeviceDesc%=rtlss.Dev, USB\VID_0BDA&PID_8170&REV_0200
%RTL8188CE_VAU.DeviceDesc%=rtlss.Dev, USB\VID_0BDA&PID_8170
%RTL8188CE_VAU.DeviceDesc%=rtlss.Dev, USB\VID_0BDA&PID_817E&REV_0200
%RTL8188CE_VAU.DeviceDesc%=rtlss.Dev, USB\VID_0BDA&PID_817E
%RTL8188CE_VAU.DeviceDesc%=rtlss.Dev, USB\VID_13D3&PID_3359
%RTL8188CE_VAU.DeviceDesc%=rtlss.Dev, USB\VID_13D3&PID_3358
; 8192CE_VAU
%RTL8192CE_VAU.DeviceDesc%=rtlss.Dev, USB\VID_0BDA&PID_817C&REV_0200
%RTL8192CE_VAU.DeviceDesc%=rtlss.Dev, USB\VID_0BDA&PID_817C
; 8188CUS-Slim Solo
%RTL8188CU_Slim_Solo.DeviceDesc%=rtlss.Dev, USB\VID_0BDA&PID_817A&REV_0200
%RTL8188CU_Slim_Solo.DeviceDesc%=rtlss.Dev, USB\VID_0BDA&PID_817A
; 8188CUS-Slim Combo
%RTL8188CU_Slim_Combo.DeviceDesc%=rtlss.Dev, USB\VID_0BDA&PID_817B&REV_0200
%RTL8188CU_Slim_Combo.DeviceDesc%=rtlss.Dev, USB\VID_0BDA&PID_817B
; Add other product in the future
%RTL8192CU.DeviceDesc%=rtlss.Dev, USB\VID_0BDA&PID_8192

; For XP and later
[Microsoft.NTx86]
%RTL8188SU.DeviceDesc%=rtlss.Dev, USB\VID_0BDA&PID_8171&REV_0200
%RTL8188SU.DeviceDesc%=rtlss.Dev, USB\VID_1690&PID_0752&REV_0200
%RTL8191SU.DeviceDesc%=rtlss.Dev, USB\VID_0BDA&PID_8172&REV_0200
%RTL8191SU.DeviceDesc%=rtlss.Dev, USB\VID_13D3&PID_3309
%RTL8191SU.DeviceDesc%=rtlss.Dev, USB\VID_13D3&PID_3339
%RTL8191SU.DeviceDesc%=rtlss.Dev, USB\VID_13D3&PID_3340
%RTL8191SU.DeviceDesc%=rtlss.Dev, USB\VID_13D3&PID_3341
%RTL8192GU.DeviceDesc%=rtlss.Dev, USB\VID_0BDA&PID_8173&REV_0200
%RTL8192SU.DeviceDesc%=rtlss.Dev, USB\VID_0BDA&PID_8174&REV_0200
; Add CU series UPDATE TO DID table V38
; 8188CUS
%RTL8188CU.DeviceDesc%=rtlss.Dev, USB\VID_0BDA&PID_8176&REV_0200
%RTL8188CU.DeviceDesc%=rtlss.Dev, USB\VID_0BDA&PID_8176
%RTL8188CU.DeviceDesc%=rtlss.Dev, USB\VID_0BDA&PID_8177&REV_0200
%RTL8188CU.DeviceDesc%=rtlss.Dev, USB\VID_0BDA&PID_8177
%RTL8188CU.DeviceDesc%=rtlss.Dev, USB\VID_2019&PID_ED17
%RTL8188CU.DeviceDesc%=rtlss.Dev, USB\VID_0DF6&PID_0052
%RTL8188CU.DeviceDesc%=rtlss.Dev, USB\VID_7392&PID_7811
%RTL8188CU.DeviceDesc%=rtlss.Dev, USB\VID_07B8&PID_8189
%RTL8188CU.DeviceDesc%=rtlss.Dev, USB\VID_0EB0&PID_9071
%RTL8188CU.DeviceDesc%=rtlss.Dev, USB\VID_06F8&PID_E033
%RTL8188CU.DeviceDesc%=rtlss.Dev, USB\VID_103C&PID_1629
%RTL8188CU.DeviceDesc%=rtlss.Dev, USB\VID_2001&PID_3308
%RTL8188CU.DeviceDesc%=rtlss.Dev, USB\VID_050D&PID_1102
%RTL8188CU.DeviceDesc%=rtlss.Dev, USB\VID_2019&PID_AB2A
%RTL8188CU.DeviceDesc%=rtlss.Dev, USB\VID_20F4&PID_648B
%RTL8188CU.DeviceDesc%=rtlss.Dev, USB\VID_4855&PID_0090
;8192 CU
%RTL8192CU.DeviceDesc%=rtlss.Dev, USB\VID_0BDA&PID_8178&REV_0200
%RTL8192CU.DeviceDesc%=rtlss.Dev, USB\VID_0BDA&PID_8178
%RTL8192CU.DeviceDesc%=rtlss.Dev, USB\VID_2001&PID_3307
%RTL8192CU.DeviceDesc%=rtlss.Dev, USB\VID_2001&PID_330A
%RTL8192CU.DeviceDesc%=rtlss.Dev, USB\VID_2001&PID_3309
%RTL8192CU.DeviceDesc%=rtlss.Dev, USB\VID_0586&PID_341F
%RTL8192CU.DeviceDesc%=rtlss.Dev, USB\VID_7392&PID_7822
%RTL8192CU.DeviceDesc%=rtlss.Dev, USB\VID_2019&PID_AB2B
%RTL8192CU.DeviceDesc%=rtlss.Dev, USB\VID_07B8&PID_8178
%RTL8192CU.DeviceDesc%=rtlss.Dev, USB\VID_07AA&PID_0056
%RTL8192CU.DeviceDesc%=rtlss.Dev, USB\VID_4855&PID_0091
;8188 RU
%RTL8188RU.DeviceDesc%=rtlss.Dev, USB\VID_0BDA&PID_817D&REV_0200
%RTL8188RU.DeviceDesc%=rtlss.Dev, USB\VID_0BDA&PID_817D
; 8188CE_VAU
%RTL8188CE_VAU.DeviceDesc%=rtlss.Dev, USB\VID_0BDA&PID_8170&REV_0200
%RTL8188CE_VAU.DeviceDesc%=rtlss.Dev, USB\VID_0BDA&PID_8170
%RTL8188CE_VAU.DeviceDesc%=rtlss.Dev, USB\VID_0BDA&PID_817E&REV_0200
%RTL8188CE_VAU.DeviceDesc%=rtlss.Dev, USB\VID_0BDA&PID_817E
%RTL8188CE_VAU.DeviceDesc%=rtlss.Dev, USB\VID_13D3&PID_3359
%RTL8188CE_VAU.DeviceDesc%=rtlss.Dev, USB\VID_13D3&PID_3358
; 8192CE_VAU
%RTL8192CE_VAU.DeviceDesc%=rtlss.Dev, USB\VID_0BDA&PID_817C&REV_0200
%RTL8192CE_VAU.DeviceDesc%=rtlss.Dev, USB\VID_0BDA&PID_817C
; 8188CUS-Slim Solo
%RTL8188CU_Slim_Solo.DeviceDesc%=rtlss.Dev, USB\VID_0BDA&PID_817A&REV_0200
%RTL8188CU_Slim_Solo.DeviceDesc%=rtlss.Dev, USB\VID_0BDA&PID_817A
; 8188CUS-Slim Combo
%RTL8188CU_Slim_Combo.DeviceDesc%=rtlss.Dev, USB\VID_0BDA&PID_817B&REV_0200
%RTL8188CU_Slim_Combo.DeviceDesc%=rtlss.Dev, USB\VID_0BDA&PID_817B
; Add other product in the future
%RTL8192CU.DeviceDesc%=rtlss.Dev, USB\VID_0BDA&PID_8192



; ============== Sections for RT SSNDIS Device ===========
[rtlss.Dev.NT]
CopyFiles=rtlss.Files.Ext

[rtlss.Dev.NT.HW]
AddReg = Enum_UpperFilter_Reg, SS_Reg

[Enum_UpperFilter_Reg]
HKR, ,  UpperFilters,  0x00010000, "rtlss"

[SS_Reg]
HKR,,"DefaultIdleTimeout",0x00010001,3000

[rtlss.Dev.NT.Services]
Addservice = rtlss, %SPSVCINST_ASSOCSERVICE%, rtlss.AddService


[rtlss.AddService]
DisplayName    = %rtlss.SvcDesc%
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  ; SERVICE_ERROR_NORMAL
ServiceBinary  = %10%\System32\Drivers\rtlss.sys
LoadOrderGroup = Base

[rtlss.Files.Ext]
rtlss.sys

[SourceDisksNames]
1=%Disk_Description%,,,

[SourceDisksFiles]
rtlss.sys = 1

[DestinationDirs]
DefaultDestDir = 12

[rtlss.Dev.NT.Remove.Services]
DelService = rtlss, 0x200

;-------------- WDF Coinstaller installation

[DestinationDirs]
CoInstaller_CopyFiles = 11

[osrusbfx2.Dev.NT.CoInstallers]
AddReg=CoInstaller_AddReg
CopyFiles=CoInstaller_CopyFiles

[CoInstaller_CopyFiles]
WdfCoInstaller01009.dll

[SourceDisksFiles]
WdfCoInstaller01009.dll=1 ; make sure the number matches with SourceDisksNames

[CoInstaller_AddReg]
HKR,,CoInstallers32,0x00010000, "WdfCoInstaller01009.dll,WdfCoInstaller"

[osrusbfx2.Dev.NT.Wdf]
KmdfService = osrusbfx2, osrusbfx2_wdfsect
[osrusbfx2_wdfsect]
KmdfLibraryVersion = 1.9

;---------------------------------------------------------------;

[Strings]
MfgName="Realtek"
Disk_Description="Installation Disk"
ClassName="USB Device"
SPSVCINST_ASSOCSERVICE= 0x00000002
RTL8188SU.DeviceDesc="Realtek RTL8188SU Selective Suspend Enabler"
RTL8191SU.DeviceDesc="Realtek RTL8191SU Selective Suspend Enabler"
RTL8192GU.DeviceDesc="Realtek RTL8192GU Selective Suspend Enabler"
RTL8192SU.DeviceDesc="Realtek RTL8192SU Selective Suspend Enabler"
RTL8188CU.DeviceDesc="Realtek RTL8188CU Selective Suspend Enabler"
RTL8192CU.DeviceDesc="Realtek RTL8192CU Selective Suspend Enabler"
RTL8188RU.DeviceDesc="Realtek RTL8188RU Selective Suspend Enabler"
RTL8188CE_VAU.DeviceDesc="Realtek RTL8188CE_VAU Selective Suspend Enabler"
RTL8192CE_VAU.DeviceDesc="Realtek RTL8192CE_VAU Selective Suspend Enabler"
RTL8188CU_Slim_Solo.DeviceDesc="Realtek RTL8188 Slim Solo_VAU Selective Suspend Enabler"
RTL8188CU_Slim_Combo.DeviceDesc="Realtek RTL8188 Slim Combo_VAU Selective Suspend Enabler"
rtlss.SvcDesc="Service for enabling selective suspend to RTL device"


