Home > Troubleshooting > Clear the Paper Jam > Paper is Jammed inside the Machine

### Paper is Jammed inside the Machine

If the machine's control panel or the Status Monitor displays there is a jam inside the machine, do the following steps.

CAUTION
  Do not attempt to remove a paper jammed deeply inside the product, particularly a paper wrapped around a heat roller. Otherwise, it may cause injuries or burns, and even worse, may generate smoke if you keep operating the product with a paper jammed. Switch off the product promptly and contact your local Fuji Xerox representative for more information.

1. Leave the machine turned on for 10 minutes for the internal fan to cool the extremely hot parts inside the machine.
2. Open the front cover.
3. Remove the toner cartridge and drum unit assembly.
   WARNING
     HOT SURFACE

     Internal parts of the machine will be extremely hot. Wait for the machine to cool down before you touch the internal parts of the machine.

4. Pull out the jammed paper slowly.
5. Install the toner cartridge and drum unit assembly into the machine.
6. Close the front cover of the machine.

Related Information
  - Clear the Paper Jam

Go to top of page