#This is the Connect Configuration file

############################################################################################
#           ---- Assist Source Settings ---
#
# - UP_enable - Supl enable
#       0 = disable
#       1 = enable
#       
# - EE_enable - Extended Eph(RXN) enable
#       0 = disable
#       1 = enable
# 
# - CP_enable - Control Plane enable
#       0 = disable
#       1 = enable
#
# - idle_secs - idle to sleep transition time in secs
#       40 = idle to sleep transition enabled
#       0 = disable
#
# - en_multi_src4app - is multisource enabled
#       0 = disable
#       1 = enable
#
# - EE_prefer - set the preference val to EE
#       0 = high
#       2^32 -1 =lowest
#
# - UP_prefer - set the preference val to UP
#       0 = high
#       2^32 -1 =lowest
#
# - Note:
#   a) If UP & EE is enabled, and if UP is given higher priority, then:
#      for cold-starts - assistance will be requested from UP only
#      for warm-starts - assistance (EPH) will be requested from both 
#                        UP and EE simultaneously
#
#   b) If UP & EE is enabled, and if EE is given higher priority, then:
#      assistance will be requested from EE and UP simultaneously
#
###########################################################################################
UP_enable=1
EE_enable=1
CP_enable=0
idle_secs=2
en_multi_src4app=1
EE_prefer=1
UP_prefer=2
############################################################################################

