;; netrtwlanu.inf 
;;
;; Realtek Wireless 802.11b/g/n USB 2.0 Network Adapter
;;
;; Copyright (C) 2011 Realtek Semiconductor Corp.
;;
;; This release is primarily for WHQL test.
;;

;FOR XP/Vista/Win7/Win8

[Version]
Signature	= "$Windows NT$"
Class		= Net
ClassGUID	= {4d36e972-e325-11ce-bfc1-08002be10318}
Provider	= %Realtek%
CatalogFile.NT	= netrtwlanu.cat		;; for WHQL certified
DriverVer = 04/13/2012,1016.1.0413.2012

[Manufacturer]
%Realtek% = Realtek,NTx86.6.1
%PCI% = PCI,NTx86.6.1
%Abocom% = Abocom,NTx86.6.1
%DLink% = DLink,NTx86.6.1
%Belkin% = Belkin,NTx86.6.1
%TRENDnet% = TRENDnet,NTx86.6.1

[ControlFlags]
ExcludeFromSelect = *



[Realtek.NTx86.6.1]
;; For 8192D RTK common		================================================================
%RTL8192du.DeviceDesc% = RTL8192du.ndi, USB\VID_0BDA&PID_8194
%RTL8192du.DeviceDesc%  = RTL8192du.ndi, USB\VID_0BDA&PID_8111
%RTL8192du0.DeviceDesc% = RTL8192du0.ndi, USB\VID_0BDA&PID_8193&MI_00
%RTL8192du1.DeviceDesc% = RTL8192du1.ndi, USB\VID_0BDA&PID_8193&MI_01
%RTL8192du2.DeviceDesc% = RTL8192du0.ndi, USB\VID_0BDA&PID_0193&MI_00
%RTL8192du3.DeviceDesc% = RTL8192du1.ndi, USB\VID_0BDA&PID_0193&MI_01

[PCI.NTx86.6.1]
;; For 8192D Customerize	================================================================
%PCI_Abocom_du0.DeviceDesc% = RTL8192du0.ndi, USB\VID_2019&PID_AB2C&MI_00
%PCI_Abocom_du1.DeviceDesc% = RTL8192du1.ndi, USB\VID_2019&PID_AB2C&MI_01
%PCI_3_du0.DeviceDesc% = RTL8192du0.ndi, USB\VID_2019&PID_4903&MI_00
%PCI_3_du1.DeviceDesc% = RTL8192du1.ndi, USB\VID_2019&PID_4903&MI_01
%PCI_4_du0.DeviceDesc% = RTL8192du0.ndi, USB\VID_2019&PID_4904&MI_00
%PCI_4_du1.DeviceDesc% = RTL8192du1.ndi, USB\VID_2019&PID_4904&MI_01
%PCIWIDI_92DU.DeviceDesc% = RTL8192du.ndi, USB\VID_2019&PID_AB2D



[Abocom.NTx86.6.1]
;; For 8192D Customerize	================================================================
%Abocom_92DU0.DeviceDesc% = RTL8192du0.ndi, USB\VID_07B8&PID_8193&MI_00
%Abocom_92DU1.DeviceDesc% = RTL8192du1.ndi, USB\VID_07B8&PID_8193&MI_01



[DLink.NTx86.6.1]
%DLink-DWA151.DeviceDesc% = DWA151.ndi, USB\VID_2001&PID_330C

[Belkin.NTx86.6.1]

%Belkin-N600DB.DeviceDesc% = BelkinN600.ndi, USB\VID_050D&PID_110A
%Belkin-N450DB.DeviceDesc% = BelkinN450.ndi, USB\VID_050D&PID_1105
%Belkin-N300DB.DeviceDesc% = BelkinN300.ndi, USB\VID_050D&PID_120A 



[TRENDnet.NTx86.6.1]
;; For 8192D Customerize	================================================================
%TRENDnet_3_du.DeviceDesc% = RTL8192du.ndi, USB\VID_20F4&PID_664B












;;----------------------------------------------------------------------------
;; Realtek 8192DU default installation
;;----------------------------------------------------------------------------


[RTL8192du.ndi.NT]
AddReg			= RTL8192du.reg, RTL8192du.common.reg, UsbRxAggrSettingOS60.reg, RateAdaptiveAndIbssSetting.reg, RTLWLAN.reg, ParticularSettingOS60.reg, CIHVS.reg, 2G40MHzAnd5G40MHz.reg
Characteristics	= 0x84
BusType			= 15 
CopyFiles		= RTWlanU.CopyFiles
*IfType			= 71            ; IF_TYPE_IEEE80211
*MediaType		= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[RTL8192du.ndi.NT.Services]
AddService		= RTL8192cu, 2, RTL8192cu.Service, RTL8192cu.EventLog
Include = netvwifibus.inf
Needs = VWiFiBus.Services

[RTL8192du.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration

[RTL8192du0.ndi.NT]
AddReg			= RTL8192du.reg, RTL8192du.common.reg, UsbRxAggrSettingOS60.reg, RateAdaptiveAndIbssSetting.reg, RTLWLAN.reg, ParticularSettingOS60.reg, CIHVS.reg, 2G40MHzAnd5G40MHz.reg
Characteristics	= 0x84
BusType			= 15 
CopyFiles		= RTWlanU.CopyFiles
*IfType			= 71            ; IF_TYPE_IEEE80211
*MediaType		= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[RTL8192du0.ndi.NT.Services]
AddService		= RTL8192cu, 2, RTL8192cu.Service, RTL8192cu.EventLog
Include = netvwifibus.inf
Needs = VWiFiBus.Services

[RTL8192du0.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration

[RTL8192du1.ndi.NT]
AddReg			= RTL8192du.reg, RTL8192du.common.reg, UsbRxAggrSettingOS60.reg, RateAdaptiveAndIbssSetting.reg, RTLWLAN.reg, ParticularSettingOS60.reg, CIHVS.reg, ConcurrentMode.reg, 2G40MHzAnd5G40MHz.reg
Characteristics	= 0x84
BusType			= 15 
CopyFiles		= RTWlanU.CopyFiles
*IfType			= 71            ; IF_TYPE_IEEE80211
*MediaType		= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[RTL8192du1.ndi.NT.Services]
AddService		= RTL8192cu, 2, RTL8192cu.Service, RTL8192cu.EventLog
Include = netvwifibus.inf
Needs = VWiFiBus.Services

[RTL8192du1.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration



;;8192D-VS Belkin Custom setting
;; Belkin N600DB suport 5G 40MHz, 2.4G 40MHz


[BelkinN600.ndi.NT]
AddReg			= RTL8192du.reg, RTL8192du.common.reg, UsbRxAggrSettingOS60.reg, RateAdaptiveAndIbssSetting.reg, RTLWLAN.reg, ParticularSettingOS60.reg, CIHVS.reg, 2G40MHzAnd5G40MHz.reg, BelkinCustomId.reg, Belkin.reg, BandSet.reg
Characteristics	= 0x84
BusType			= 15 
CopyFiles		= RTWlanU.CopyFiles
*IfType			= 71            ; IF_TYPE_IEEE80211
*MediaType		= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[BelkinN600.ndi.NT.Services]
AddService		= RTL8192cu, 2, RTL8192cu.Service, RTL8192cu.EventLog
Include = netvwifibus.inf
Needs = VWiFiBus.Services

[BelkinN600.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration


;;Belkin N450DB support 2.4G 20MHz, 5G 40MHz


[BelkinN450.ndi.NT]
AddReg			= RTL8192du.reg, RTL8192du.common.reg, UsbRxAggrSettingOS60.reg, RateAdaptiveAndIbssSetting.reg, RTLWLAN.reg, ParticularSettingOS60.reg, CIHVS.reg, 2G20MHzAnd5G40MHz.reg, BelkinCustomId.reg, Belkin.reg, BandSet.reg
Characteristics	= 0x84
BusType			= 15 
CopyFiles		= RTWlanU.CopyFiles
*IfType			= 71            ; IF_TYPE_IEEE80211
*MediaType		= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[BelkinN450.ndi.NT.Services]
AddService		= RTL8192cu, 2, RTL8192cu.Service, RTL8192cu.EventLog
Include = netvwifibus.inf
Needs = VWiFiBus.Services

[BelkinN450.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration


;;BelkinN300DB support 2.4G 20MHz, 5G 20MHz


[BelkinN300.ndi.NT]
AddReg			= RTL8192du.reg, RTL8192du.common.reg, UsbRxAggrSettingOS60.reg, RateAdaptiveAndIbssSetting.reg, RTLWLAN.reg, ParticularSettingOS60.reg, CIHVS.reg, 2G20MHzAnd5G20MHz.reg, BelkinCustomId.reg, Belkin.reg, BandSet.reg
Characteristics	= 0x84
BusType			= 15 
CopyFiles		= RTWlanU.CopyFiles
*IfType			= 71            ; IF_TYPE_IEEE80211
*MediaType		= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[BelkinN300.ndi.NT.Services]
AddService		= RTL8192cu, 2, RTL8192cu.Service, RTL8192cu.EventLog
Include = netvwifibus.inf
Needs = VWiFiBus.Services

[BelkinN300.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration

;;End of 8192D-VS Belkin Custom setting


;;8192D-VS Dlink DWA151 Custom setting
;; DWA151 configure 2x2 to 1x1 


[DWA151.ndi.NT]
AddReg			= RTL8192du.reg, RTL8192du.common.reg, UsbRxAggrSettingOS60.reg, RateAdaptiveAndIbssSetting.reg, RTLWLAN.reg, ParticularSettingOS60.reg, CIHVS.reg, 2G40MHzAnd5G40MHz.reg,SMSPSuppot1by1.reg
Characteristics	= 0x84
BusType			= 15 
CopyFiles		= RTWlanU.CopyFiles
*IfType			= 71            ; IF_TYPE_IEEE80211
*MediaType		= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[DWA151.ndi.NT.Services]
AddService		= RTL8192cu, 2, RTL8192cu.Service, RTL8192cu.EventLog
Include = netvwifibus.inf
Needs = VWiFiBus.Services

[DWA151.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration

;;End of 8192D-VS Dlink DWA151 Custom setting







[RTL8192cu.Service]
DisplayName    = %RTL8192cu.DeviceDesc.DispName%
ServiceType    = 1		; %SERVICE_KERNEL_DRIVER%
StartType      = 3		; %SERRVICE_DEMAND_START%
ErrorControl   = 1		; %SERRVICE_ERROR_NORMAL%
ServiceBinary  = %12%\rtwlanu.sys
LoadOrderGroup = NDIS

[RTL8192cu.EventLog]
AddReg = RTL8192cu.AddEventLog.reg

[RTL8192cu.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported  , 0x00010001, 7



[RTL8192du.reg]
HKR, Ndi\Interfaces,	UpperRange, 0, "ndis5,mdcwifi"
HKR, Ndi\Interfaces,	LowerRange, 0, "wlan, ethernet, vwifi"
HKR, Ndi,				Service,    0, "RTL8192du"



;*******************************************************************************
; RTL8192du common paramters
;*******************************************************************************
[RTL8192du.common.reg]
HKR,defaults,LedCtrl,0,"1"
HKR,,LedCtrl,0,"1"

HKR,defaults,QoS,0,"1"
HKR,,QoS,0,"1"

;; For Earlymode 1:Enable 0:Disable
HKR,,bEarlymodeEnable,,"1"

HKR,defaults,CcxRm,0,"1"
HKR,,CcxRm,0,"1"

HKR,defaults,CcxOffLineDurUpLimit,0,"0"
HKR,,CcxOffLineDurUpLimit,0,"0"

;-------------------------------------------------------------------------------
;	USB Tx/Rx aggregation
;-------------------------------------------------------------------------------
HKR,defaults,UsbRxAggBlockCount,0,"18"
HKR,,UsbRxAggBlockCount,0,"18"

HKR,defaults,UsbRxAggBlockTimeout,0,"7"
HKR,,UsbRxAggBlockTimeout,0,"7"

HKR,defaults,UsbRxAggPageTimeout,0,"6"
HKR,,UsbRxAggPageTimeout,0,"6"

HKR,defaults,UsbTxAggMode,0,"1"
HKR,,UsbTxAggMode,0,"1"

HKR,defaults,UsbTxAggDescNum,0,"4"
HKR,,UsbTxAggDescNum,0,"4"

HKR,defaults,SupportTxPacketBufferColease,0,"0"
HKR,,SupportTxPacketBufferColease,0,"0"



[RateAdaptiveAndIbssSetting.reg]
HKR,defaults,WiFi11bIbss,0,"0"
HKR,,WiFi11bIbss,0,"0"

HKR,defaults,bRateAdaptive,0,"1"
HKR,,bRateAdaptive,0,"1"



[UsbRxAggrSettingOS60.reg]
HKR,defaults,UsbRxAggMode,0,"2"
HKR,,UsbRxAggMode,0,"2"

HKR,defaults,UsbRxAggPageCount,0,"16"
HKR,,UsbRxAggPageCount,0,"16"

;;----------------------------------------------------------------------------
;; Realtek WLAN NIC parameters
;;----------------------------------------------------------------------------
[RTLWLAN.reg]
HKR,defaults,SSID,0,"ANY"
HKR,,SSID,0,"ANY"

HKR,defaults,Channel,0,"1"
HKR,,Channel,0,"1"

HKR,Ndi\params\NetworkType,			ParamDesc,  0, %NETWORK_TYPE_STR%
HKR,Ndi\params\NetworkType,			type,       0, "enum"
HKR,Ndi\params\NetworkType,			default,    0, "1"
HKR,Ndi\params\NetworkType\enum,		"0",        0, %AD_HOC_STR%
HKR,Ndi\params\NetworkType\enum,		"1",        0, %INFRASTRUCTURE_STR%
HKR,Ndi\params\NetworkType\enum,		"2",        0, %AUTO_SELECT%
HKR,defaults,NetworkType,0,"1"
HKR,,NetworkType,0,"1"

HKR,defaults,StaUapsd,0,"0"
HKR,,StaUapsd,0,"0"

; For B/G mode and B/G/N mode switch, we will use different wireless mode registry in later section
;HKR,Ndi\params\WirelessMode, 			ParamDesc, 	0, %WL_MODE_STR%
;HKR,Ndi\params\WirelessMode, 			type, 		0, "enum"
;HKR,Ndi\params\WirelessMode, 			default, 	0, "8"
;HKR,Ndi\params\WirelessMode\enum, 		"2", 		0, %IEEE_802_11B_STR%
;HKR,Ndi\params\WirelessMode\enum, 		"4", 		0, %IEEE_802_11BG_STR%
;HKR,Ndi\params\WirelessMode\enum, 		"8", 		0, %IEEE_802_11BGN_STR%
;HKR,defaults,WirelessMode, 0, "8"
;HKR,,WirelessMode, 0, "8"

;; For WiFi test, 1: WiFi Config and 0: Performance Config
HKR,Ndi\params\WiFiConfg,        ParamDesc,  0, "WiFi Config"
HKR,Ndi\params\WiFiConfg,        type,       0, "enum"
HKR,Ndi\params\WiFiConfg,        default,    0, "0"
HKR,Ndi\params\WiFiConfg\enum,   "0",        0, "Performance"
HKR,Ndi\params\WiFiConfg\enum,   "1",        0, "WiFi"
HKR,defaults,WiFiConfg,0,"0"
HKR,,WiFiConfg,0,"0"
HKR,,WiFiConfg,,"0"

HKR,defaults,RxReorder,0,"1"
HKR,,RxReorder,0,"1"

HKR,,DefaultKeyID,,"0"
HKR,,DefaultKey0,,""
HKR,,DefaultKey1,,""
HKR,,DefaultKey2,,""
HKR,,DefaultKey3,,""

;Leisure Power Save
HKR,defaults,bLeisurePs,0,"2"
HKR,,bLeisurePs,0,"2"

;Fw Control LPS
HKR,defaults,bFwCtrlLPS,0,"3"
HKR,,bFwCtrlLPS,0,"3"

;; LPS Interval
;HKR,defaults,LPSIntvl,0,"5"
HKR,,LPSIntvl,0,"5"

;BTmode
HKR,,bBTMode,0,"1"

; Reset Tx Hang
HKR,defaults,USBResetTxHang,0,"1"
HKR,,USBResetTxHang,0,"1"

HKR,,WEPinNmode,0,"0"

;-------------------------------------------------------------------------------
;	Some function ability setting
;-------------------------------------------------------------------------------

HKR,defaults,UPDMEnable,0,"1"
HKR,,UPDMEnable,0,"1"

HKR,defaults,LinkSpeedLevel,0,"0"
HKR,,LinkSpeedLevel,0,"0"

HKR,defaults,AutoConnect,0,"1"
HKR,,AutoConnect,0,"1"

HKR,defaults,RWRetry,0,"0"
HKR,,RWRetry,0,"0"

HKR,defaults,MultiMode,0,"1"
HKR,,MultiMode,0,"1"

HKR,defaults,TxMode,0,"0"
HKR,,TxMode,0,"0"

HKR,defaults,GainOffsetMKKLow,0,"0"
HKR,,GainOffsetMKKLow,0,"0"
HKR,defaults,GainOffsetMKK,0,"0"
HKR,,GainOffsetMKK,0,"0"
HKR,defaults,GainOffsetMKKHigh,0,"0"
HKR,,GainOffsetMKKHigh,0,"0"

HKR,defaults,GainOffsetETSILow,0,"0"
HKR,,GainOffsetETSILow,0,"0"
HKR,defaults,GainOffsetETSI,0,"0"
HKR,,GainOffsetETSI,0,"0"
HKR,defaults,GainOffsetETSIHigh,0,"0"
HKR,,GainOffsetETSIHigh,0,"0"

HKR,defaults,RxSC,0,"0"
HKR,,RxSC,0,"0"

HKR,defaults,TxSC,0,"0"
HKR,,TxSC,0,"0"



HKR,defaults,MaxBINumber,0,"10"
HKR,,MaxBINumber,0,"10"


[ParticularSettingOS60.reg]
;Inactive Power Save
HKR,defaults,InactivePs,0,"2"
HKR,,InactivePs,0,"2"

HKR,defaults,AggDMEnable,0,"1"
HKR,,AggDMEnable,0,"1"

; /****************************************************************************
; ** IHV Service Reg for CCX
; ****************************************************************************/
[CIHVS.reg]
HKR, Ndi\IHVExtensions, ExtensibilityDLL,       0,  "%SystemRoot%\system32\Rtlihvs.dll"
HKR, Ndi\IHVExtensions, UIExtensibilityCLSID,   0,  "{6C2A8CCA-B2A2-4d81-A3B2-4E15F445C312}"
HKR, Ndi\IHVExtensions, GroupName,              0,  "Realtek CCX SDK IHV Service"
HKR, Ndi\IHVExtensions, AdapterOUI,             0x00010001, 0x00e04c

;;----------------------------------------------------------------------------
;; Belkin WLAN NIC parameters
;;----------------------------------------------------------------------------
[Belkin.reg]
HKR,Ndi\params\RFOff,			ParamDesc,  0, "Radio"
HKR,Ndi\params\RFOff,			type,       0, "enum"
HKR,Ndi\params\RFOff,			default,    0, "0"
HKR,Ndi\params\RFOff\enum,		"0",        0, "On"
HKR,Ndi\params\RFOff\enum,		"1",        0, "Off"
HKR,defaults,RFOff,0,"0"
HKR,,RFOff,0,"0"

;;----------------------------------------------------------------------------
;; Wireless mode option parameters
;;----------------------------------------------------------------------------
[11gWirelessMode.reg]
HKR,Ndi\params\WirelessMode, 		ParamDesc, 	0, %WL_MODE_STR%
HKR,Ndi\params\WirelessMode, 		type, 		0, "enum"
HKR,Ndi\params\WirelessMode, 		default, 	0, "8"
HKR,Ndi\params\WirelessMode\enum, 	"2", 		0, %IEEE_802_11B_STR%
HKR,Ndi\params\WirelessMode\enum, 	"4", 		0, %IEEE_802_11BG_STR%
HKR,defaults,WirelessMode, 0, "4"
HKR,,WirelessMode, 0, "4"





;*******************************************************************************
; Two STA Concurrent Mode Reg
;*******************************************************************************
[ConcurrentMode.reg]
HKR,Ndi\params\TwoStaConcurrentMode,		ParamDesc,  0, %TWO_STA_CONCURRENT_MODE%
HKR,Ndi\params\TwoStaConcurrentMode,		type,       0, "enum"
HKR,Ndi\params\TwoStaConcurrentMode,			default,    0, "1"
HKR,Ndi\params\TwoStaConcurrentMode\enum,		"0",        0, %SECONDARY_DISABLE%
HKR,Ndi\params\TwoStaConcurrentMode\enum,		"1",        0, %SECONDARY_ENABLE%
HKR,Ndi\params\TwoStaConcurrentMode\enum,		"2",        0, %SECONDARY_AUTO%
HKR,defaults,TwoStaConcurrentMode,0,"0"
HKR,,TwoStaConcurrentMode,0,"0"

;*******************************************************************************
; 8192DU-VS 2.4G/5G 40MHz Support
;*******************************************************************************
[2G40MHzAnd5G40MHz.reg]
HKR,Ndi\params\BW40MHzFor2G,        ParamDesc,  0, "Bandwidth_2.4G"
HKR,Ndi\params\BW40MHzFor2G,        type,       0, "enum"
HKR,Ndi\params\BW40MHzFor2G,        default,    0, "1"
HKR,Ndi\params\BW40MHzFor2G\enum,   "0",        0, "20MHz Only"
HKR,Ndi\params\BW40MHzFor2G\enum,   "1",        0, "20_40MHz"
HKR,defaults,BW40MHzFor2G,0,"1"
HKR,,BW40MHzFor2G,0,"1"
HKR,,BW40MHzFor2G,,"1"

HKR,Ndi\params\BW40MHzFor5G,        ParamDesc,  0, "Bandwidth_5G"
HKR,Ndi\params\BW40MHzFor5G,        type,       0, "enum"
HKR,Ndi\params\BW40MHzFor5G,        default,    0, "1"
HKR,Ndi\params\BW40MHzFor5G\enum,   "0",        0, "20MHz Only"
HKR,Ndi\params\BW40MHzFor5G\enum,   "1",        0, "20_40MHz"
HKR,defaults,BW40MHzFor5G,0,"1"
HKR,,BW40MHzFor5G,0,"1"
HKR,,BW40MHzFor5G,,"1"

[2G20MHzAnd5G40MHz.reg]
HKR,defaults,BW40MHzFor2G,0,"0"
HKR,,BW40MHzFor2G,0,"0"

HKR,Ndi\params\BW40MHzFor5G,        ParamDesc,  0, "Bandwidth_5G"
HKR,Ndi\params\BW40MHzFor5G,        type,       0, "enum"
HKR,Ndi\params\BW40MHzFor5G,        default,    0, "1"
HKR,Ndi\params\BW40MHzFor5G\enum,   "0",        0, "20MHz Only"
HKR,Ndi\params\BW40MHzFor5G\enum,   "1",        0, "20_40MHz"
HKR,defaults,BW40MHzFor5G,0,"1"
HKR,,BW40MHzFor5G,0,"1"
HKR,,BW40MHzFor5G,,"1"

[2G20MHzAnd5G20MHz.reg]
HKR,defaults,BW40MHzFor2G,0,"0"
HKR,,BW40MHzFor2G,0,"0"

HKR,defaults,BW40MHzFor5G,0,"0"
HKR,,BW40MHzFor5G,0,"0"

[BandWidthSetting.reg]
;; 40MHz Support in 11n
HKR,Ndi\params\BW40MHz,        ParamDesc,  0, "Bandwidth"
HKR,Ndi\params\BW40MHz,        type,       0, "enum"
HKR,Ndi\params\BW40MHz,        default,    0, "1"
HKR,Ndi\params\BW40MHz\enum,   "0",        0, "20MHz Only"
HKR,Ndi\params\BW40MHz\enum,   "1",        0, "20_40MHz"
HKR,defaults,BW40MHz,0,"1"
HKR,,BW40MHz,0,"1"
HKR,,BW40MHz,,"1"

[BelkinCustomId.reg]
HKR,,CustomerID,0,"21"
HKR,,CustomerID,,"21"

[BandSet.reg]
HKR,Ndi\params\WirelessBand,			ParamDesc,  0, "Disable Bands"
HKR,Ndi\params\WirelessBand,			type,       0, "enum"
HKR,Ndi\params\WirelessBand,			default,    0, "0"
HKR,Ndi\params\WirelessBand\enum,		"0",        0, "Disable 11A"
HKR,Ndi\params\WirelessBand\enum,		"1",        0, "Disable 11B/G"
HKR,Ndi\params\WirelessBand\enum,		"2",        0, "None"
HKR,defaults,WirelessBand,0,"2"
HKR,,WirelessBand,0,"2"
;*****************************************************************************
; 92DU VS support 1x1 mode
;*****************************************************************************
[SMSPSuppot1by1.reg]
HKR,defaults,SMSP1By1,0,"1"
HKR,,SMSP1By1,0,"1"

;*******************************************************************************
; Destination Directory
;*******************************************************************************
[RTWlanU.CopyFiles]
RTWlanU.sys,,,2

[DestinationDirs]
DefaultDestDir     = 11
RTWlanU.CopyFiles		= 12

;;****************************************************************************
;; Source Files
;;****************************************************************************
[SourceDisksFiles]
RTWlanU.sys = 1

[SourceDisksNames]
1=%DISKNAME%,,,

;*******************************************************************************
; Strings
;*******************************************************************************
[Strings]
SSID_STR					= "SSID"
CHANNEL_STR				= "Channel"
NETWORK_TYPE_STR			= "Network Type"
LED_CONTROL_STR				= "LED Control" 
POWER_SAVE_STR				= "Power Save Mode"
WIFI_IBSS_STR				= "IBSS Default 11b Mode"
RATE_ADAPTIVE_STR			= "Rate Adaptive"
QOS_STR					= "QoS"
WiFiConfg_STR	  			= "WiFiConfg"
WMM_APSD				= "WMM APSD"
CCX_RM_STR				= "CCX Radio Measurement"
CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "CCX Max Off-Line Measurement (0: unlimited)"
FORCE_PRIORITY_STR			= "Forced Priority"
HW_PARA_STR				= "Init from HwParaFile"
THREE_WIRE_MODE_STR			= "Three Wire Programming Mode"
BOARD_TYPE_STR				= "Board Type"
PROTECTION_MODE_STR			= "Protection Mode"
TPC_STR					= "Transmit Power Control"
TPC_POLARITY_STR				= "TPC Polarity Select"
HIGH_POWER_STR				= "High Power Mechanism"
INIT_GAIN_STR				= "Initial Gain State"
CW_MAX_MIN_STR				= "Contention Window"
PSP_XLINK_STR				= "PSP XLink Mode"
DISABLE_STR				= "Disable"
ENABLE_STR				= "Enable"
AD_HOC_STR				= "Ad Hoc"
INFRASTRUCTURE_STR			= "Infrastructure"
AUTO_SELECT				= "Auto select"
WL_MODE_STR				= "Wireless Mode"
RX_REORDER_STR				= "Rx Reorder"
CAM_STR					= "CAM"
MAX_PSP_STR				= "MAX_PSP"
Fast_PSP_STR				= "Fast_PSP"
NO_AC_STR				= "No AC (Disable)"
ALL_AC_STR				= "ALL AC"
IEEE_802_11B_STR 				= "IEEE 802.11b"
IEEE_802_11BG_STR 				= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"

;-------------------------------------------------------------------------------
;	USB Tx/Rx aggregation strings
;-------------------------------------------------------------------------------
RX_AGG_MODE_STR				= "Rx Aggregation Mode"
RX_AGG_MODE_BLOCK_STR			= "Rx Agg USB Block Mode"
RX_AGG_MODE_PAGE_STR			= "Rx Agg DMA Page Mode"
RX_AGG_MODE_MIXED_STR			= "Rx Agg USB and Page Mixed Mode"
RX_AGG_USB_BLOCK_STR			= "Rx Agg USB Block Threshold"
RX_AGG_USB_TIMEOUT_STR			= "Rx Agg USB Timeout"
RX_AGG_DMA_PAGE_STR			= "Rx Agg DMA Page Threshold"
RX_AGG_DMA_TIMEOUT_STR			= "Rx Agg DMA Timeout"
TX_AGG_MODE_STR				= "Tx Aggregation Mode"
TX_AGG_DESC_PER_OUT_STR			= "Tx Agg Number of descriptor per bulk out"

;-------------------------------------------------------------------------------
;	Two STA Concurrent Mode
;-------------------------------------------------------------------------------
TWO_STA_CONCURRENT_MODE			= "Two STA Concurrent Mode"
SECONDARY_DISABLE			= "Secondary client Disable"
SECONDARY_ENABLE			= "Secondary Client Enable"
SECONDARY_AUTO				= "Secondary Client Auto Select"

;*******************************************************************************
; manufacture description
;*******************************************************************************
Realtek					= "Realtek Semiconductor Corp."
PCI             		= "PLANEX COMMUNICATIONS INC"
Sitecom         		= "Sitecom Europe B.V."
EDIMAX         			= "EDIMAX"
Abocom					= "AboCom System, Inc."
Amigo					= "Amigo Technology Inc"
Hercules				= "Guillemot Corporation S.A"
DLink					= "D-Link Corporation"
Belkin					= "Belkin International, Inc."
Zyxel					= "ZyXEL"
ATKK92cu				= "Allied Telesis K.K."
TRENDnet				= "TRENDnet"
Feixun92cu				= "Shanghai Feixun Communication Co.,Ltd"
Feixun_Net92cu			= "NetweeN"
XAVI					= "XAVI Technologies Corp."
Netgearcus				= "NETGEAR Inc."
Oar_Inc					= "Oar Inc."
ASUS					= "ASUSTeK Computer Inc."
HAWKING					= "Hawking Technologies Inc."
Compare					= "Compare Electronics CO.,LTD"


;*******************************************************************************
;	Source disk name
;*******************************************************************************
;DISKNAME							= "Realtek RTL8192CU Wireless LAN 802.11n USB 2.0 Network Adapter Driver Disk"
DISKNAME							= "Realtek Wireless LAN 802.11n USB 2.0 Network Adapter Driver Disk"
RTL8192cu.DeviceDesc 				= "Realtek RTL8192CU Wireless LAN 802.11n USB 2.0 Network Adapter"
RTL8192cu.DeviceDesc.DispName		= "Realtek RTL8192CU Wireless LAN 802.11n USB 2.0 Network Adapter"
RTL8188cu.DeviceDesc 				= "Realtek RTL8188CU Wireless LAN 802.11n USB 2.0 Network Adapter"
RTL8188cu.DeviceDesc.DispName		= "Realtek RTL8188CU Wireless LAN 802.11n USB 2.0 Network Adapter"
RTL8188cu_G.DeviceDesc 				= "Realtek RTL8188CU Wireless LAN 802.11 USB 2.0 Network Adapter"
RTL8188cu_G.DeviceDesc.DispName		= "Realtek RTL8188CU Wireless LAN 802.11 USB 2.0 Network Adapter"
RTL8188ce_vau.DeviceDesc 			= "Realtek RTL8188CE-VAU Wireless LAN 802.11n USB minicard"
RTL8188ce_vau.DeviceDesc.DispName	= "Realtek RTL8188CE-VAU Wireless LAN 802.11n USB minicard"
RTL8188ce_vau_G.DeviceDesc 			= "Realtek RTL8188CE-VAU Wireless LAN 802.11 USB minicard"
RTL8188ce_vau_G.DeviceDesc.DispName	= "Realtek RTL8188CE-VAU Wireless LAN 802.11 USB minicard"
RTL8192ce_vau.DeviceDesc 			= "Realtek RTL8192CE-VAU Wireless LAN 802.11n USB minicard"
RTL8192ce_vau.DeviceDesc.DispName	= "Realtek RTL8192CE-VAU Wireless LAN 802.11n USB minicard"
RTL8188cu_slim_solo.DeviceDesc		= "Realtek RTL8188CUS Wireless LAN 802.11n USB Slim Solo"
RTL8188cu_slim_solo.DeviceDesc.DispName	= "Realtek RTL8188CUS Wireless LAN 802.11n USB Slim Solo"
RTL8188cu_slim_solo_lc.DeviceDesc		= "Realtek RTL8188CUS Wireless LAN 802.11n USB Slim Solo"
RTL8188cu_slim_solo_lc.DeviceDesc.DispName	= "Realtek RTL8188CUS Wireless LAN 802.11n USB Slim Solo"
RTL8188cu_slim_combo.DeviceDesc		= "Realtek RTL8188CUS Wireless LAN 802.11n USB Slim Combo"
RTL8188cu_slim_combo.DeviceDesc.DispName= "Realtek RTL8188CUS Wireless LAN 802.11n USB Slim Combo"
RTL8188ru.DeviceDesc 				= "Realtek RTL8188RU Wireless LAN 802.11n USB High Power Dongle"
RTL8188ru.DeviceDesc.DispName		= "Realtek RTL8188RU Wireless LAN 802.11n USB High Power Dongle"
RTL8188cus_vl.DeviceDesc 			= "Realtek RTL8188CUS-VL Wireless LAN 802.11n USB 2.0 Network Adapter"
RTL8188cus_vl.DeviceDesc.DispName	= "Realtek RTL8188CUS-VL Wireless LAN 802.11n USB 2.0 Network Adapter"
RTK_AZ88vau.DeviceDesc				= "Realtek RTL8188CE-VAU Wireless LAN 802.11n USB minicard"
RTK_AZ88vau.DeviceDesc.DispName		= "Realtek RTL8188CE-VAU Wireless LAN 802.11n USB minicard"
RTK_AZ88vau_G.DeviceDesc			= "Realtek RTL8188CE-VAU Wireless LAN 802.11 USB minicard"
RTK_AZ88vau_G.DeviceDesc.DispName	= "Realtek RTL8188CE-VAU Wireless LAN 802.11 USB minicard"
RTK_AZ88cus.DeviceDesc				= "Wireless USB Card"
RTK_AZ88cus.DeviceDesc.DispName		= "Wireless USB Card"
RTL8188ctv.DeviceDesc				= "Realtek RTL8188CTV Wireless LAN 802.11n USB 2.0 Network Adapter"
RTL8188ctv.DeviceDesc.DispName		= "Realtek RTL8188CTV Wireless LAN 802.11n USB 2.0 Network Adapter"
PCI.DeviceDesc 						= "GW-USValue-EZ"
PCI.DeviceDesc.DispName				= "GW-USValue-EZ"
PCI-2.DeviceDesc 					= "GW-USLight"
PCI-2.DeviceDesc.DispName			= "GW-USLight"
PCI_Abocom88cu.DeviceDesc 			= "GW-USNano2"
PCI_Abocom88cu.DeviceDesc.DispName	= "GW-USNano2"
PCI_Abocom92cu.DeviceDesc 			= "GW-USEco300"
PCI_Abocom92cu.DeviceDesc.DispName	= "GW-USEco300"
PCI_Vencer.DeviceDesc 				= "BT-Micro3H2X Wireless LAN"
PCI_Vencer.DeviceDesc.DispName		= "BT-Micro3H2X Wireless LAN"
PCI_Abocom_du0.DeviceDesc 			= "GW-USDual300 MAC0"
PCI_Abocom_du0.DeviceDesc.DispName	= "GW-USDual300 MAC0"
PCI_Abocom_du1.DeviceDesc 			= "GW-USDual300 MAC1"
PCI_Abocom_du1.DeviceDesc.DispName	= "GW-USDual300 MAC1"
PCI_3_du0.DeviceDesc 				= "GW-USFang300 MAC0"
PCI_3_du0.DeviceDesc.DispName		= "GW-USFang300 MAC0"
PCI_3_du1.DeviceDesc 				= "GW-USFang300 MAC1"
PCI_3_du1.DeviceDesc.DispName		= "GW-USFang300 MAC1"
PCI_4_du0.DeviceDesc 				= "GW-USUltra300 MAC0"
PCI_4_du0.DeviceDesc.DispName		= "GW-USUltra300 MAC0"
PCI_4_du1.DeviceDesc 				= "GW-USUltra300 MAC1"
PCI_4_du1.DeviceDesc.DispName		= "GW-USUltra300 MAC1"
PCIWIDI_92DU.DeviceDesc 			= "MZK-WD300DH"
PCIWIDI_92DU.DeviceDesc.DispName		= "MZK-WD300DH"
Sitecom.DeviceDesc 					= "Sitecom Wireless Ultra Nano USB Adapter 150N X1 WL-365"
Sitecom.DeviceDesc.DispName			= "Sitecom Wireless Ultra Nano USB Adapter 150N X1 WL-365"
Sitecom_UN.DeviceDesc 				= "Wireless Ultra Nano Network Adapter 150N"
Sitecom_UN.DeviceDesc.DispName		= "Wireless Ultra Nano Network Adapter 150N"
Sitecom_HG.DeviceDesc 				= "Wireless High-gain Network adapter 300N WLA-4001"
Sitecom_HG.DeviceDesc.DispName		= "Wireless High-gain Network adapter 300N WLA-4001"
EDIMAX.DeviceDesc 					= "150Mbps Wireless 802.11b/g/n Nano USB Adapter"
EDIMAX.DeviceDesc.DispName			= "150Mbps Wireless 802.11b/g/n Nano USB Adapter"
EDIMAX300.DeviceDesc 				= "Edimax 300Mbps wireless 802.11b/g/n USB adapter"
EDIMAX300.DeviceDesc.DispName		= "Edimax 300Mbps wireless 802.11b/g/n USB adapter"
Abocom.DeviceDesc 					= "802.11n/b/g Mini Wireless LAN USB2.0 Adapter"
Abocom.DeviceDesc.DispName			= "802.11n/b/g Mini Wireless LAN USB2.0 Adapter"
Abocom92cu.DeviceDesc				= "802.11n/b/g Mini Wireless LAN USB2.0 Adapter"
Abocom92cu.DeviceDesc.DispName		= "802.11n/b/g Mini Wireless LAN USB2.0 Adapter"
Abocom_92DU0.DeviceDesc			= "802.11 a/b/g/n Wireless LAN USB 2.0 Network Adapter MAC0"
Abocom_92DU0.DeviceDesc.DispName	= "802.11 a/b/g/n Wireless LAN USB 2.0 Network Adapter MAC0"
Abocom_92DU1.DeviceDesc			= "802.11 a/b/g/n Wireless LAN USB 2.0 Network Adapter MAC1"
Abocom_92DU1.DeviceDesc.DispName	= "802.11 a/b/g/n Wireless LAN USB 2.0 Network Adapter MAC1"
Amigo.DeviceDesc 					= "Wireless USB Card"
Amigo.DeviceDesc.DispName			= "Wireless USB Card"
Hercules.DeviceDesc 				= "Hercules Wireless N Pico USB "
Hercules.DeviceDesc.DispName		= "Hercules Wireless N Pico USB "
DLink-1.DeviceDesc 					= "D-Link DWA-133 Wireless N USB Adapter"
DLink-1.DeviceDesc.DispName			= "D-Link DWA-133 Wireless N USB Adapter"
DLink-2.DeviceDesc 					= "D-Link DWA-135 Wireless N USB Adapter"
DLink-2.DeviceDesc.DispName			= "D-Link DWA-135 Wireless N USB Adapter"
DLink-3.DeviceDesc 					= "D-Link DWA-121 Wireless N USB Adapter"
DLink-3.DeviceDesc.DispName			= "D-Link DWA-121 Wireless N USB Adapter"
DLink-4.DeviceDesc 					= "D-Link DWA-130 Wireless N USB Adapter(rev.F1)"
DLink-4.DeviceDesc.DispName			= "D-Link DWA-130 Wireless N USB Adapter(rev.F1)"
DLink-5.DeviceDesc 					= "D-Link DWA-123 Wireless N 150 USB Adapter(rev.C)"
DLink-5.DeviceDesc.DispName			= "D-Link DWA-123 Wireless N 150 USB Adapter(rev.C)"
Belkin.DeviceDesc 					= "Surf Wireless Micro USB Adapter"
Belkin.DeviceDesc.DispName			= "Surf Wireless Micro USB Adapter"
Belkin-2.DeviceDesc 				= "Belkin Surf & Share Wireless USB Adapter"
Belkin-2.DeviceDesc.DispName		= "Belkin Surf & Share Wireless USB Adapter"
Belkin-3.DeviceDesc 				= "N300 USB Network Adapter"
Belkin-3.DeviceDesc.DispName		= "N300 USB Network Adapter"
Belkin-4.DeviceDesc 				= "Belkin Wireless Adapter"
Belkin-4.DeviceDesc.DispName		= "Belkin Wireless Adapter"
ZyXEL.DeviceDesc 					= "ZyXEL Wireless LAN 802.11n USB 2.0 Network Adapter"
ZyXEL.DeviceDesc.DispName			= "ZyXEL Wireless LAN 802.11n USB 2.0 Network Adapter"
ATKK92cu.DeviceDesc					= "Corega CG-WLUSB300NS"
ATKK92cu.DeviceDesc.DispName		= "Corega CG-WLUSB300NS"
TRENDnet.DeviceDesc					= "TRENDnet 150Mbps Micro Wireless N USB Adapter"
TRENDnet.DeviceDesc.DispName		= "TRENDnet 150Mbps Micro Wireless N USB Adapter"
TRENDnet_2.DeviceDesc				= "TRENDnet 300Mbps Mini Wireless N USB Adapter"
TRENDnet_2.DeviceDesc.DispName		= "TRENDnet 300Mbps Mini Wireless N USB Adapter"
TRENDnet_3_du.DeviceDesc			= "TRENDnet 300Mbps Dual Band Wireless N USB Adapter"
TRENDnet_3_du.DeviceDesc.DispName	= "TRENDnet 300Mbps Dual Band Wireless N USB Adapter"
Feixun92cu.DeviceDesc 				= "FEIXUN Wireless LAN 802.11n USB 2.0 Network Adaptor"
Feixun92cu.DeviceDesc.DispName		= "FEIXUN Wireless LAN 802.11n USB 2.0 Network Adaptor"
Feixun_Net92cu.DeviceDesc 			= "NetweeN Wireless LAN 802.11n USB 2.0 Network Adaptor"
Feixun_Net92cu.DeviceDesc.DispName	= "NetweeN Wireless LAN 802.11n USB 2.0 Network Adaptor"
XAVI.DeviceDesc 					= "Realtek RTL8188CUS Wireless LAN 802.11n USB Slim Solo"
XAVI.DeviceDesc.DispName			= "Realtek RTL8188CUS Wireless LAN 802.11n USB Slim Solo"
XAVI88cusc.DeviceDesc 				= "Realtek RTL8188CUS Wireless LAN 802.11n USB Slim Combo"
XAVI88cusc.DeviceDesc.DispName		= "Realtek RTL8188CUS Wireless LAN 802.11n USB Slim Combo"
Netgearcus.DeviceDesc 				= "NETGEAR WNA1000M N150 Wireless USB Micro Adapter"
Netgearcus.DeviceDesc.DispName		= "NETGEAR WNA1000M N150 Wireless USB Micro Adapter"
Oar_Inc.DeviceDesc 					= "SW-WF02-AD15"
Oar_Inc.DeviceDesc.DispName			= "SW-WF02-AD15"
ASUS.DeviceDesc 					= "ASUS USB-N13 300Mbps 11n Wireless USB dongle"
ASUS.DeviceDesc.DispName			= "ASUS USB-N13 300Mbps 11n Wireless USB dongle"
Hawking-1.DeviceDesc 				= "Hawking HWDN3 Wls-N Dish Adapter"
Hawking-1.DeviceDesc.DispName		= "Hawking HWDN3 Wls-N Dish Adapter"
Hawking-2.DeviceDesc 				= "Hawking HWUN4 Wls-300N Adapter"
Hawking-2.DeviceDesc.DispName		= "Hawking HWUN4 Wls-300N Adapter"
Compare-1.DeviceDesc 				= "Compare Wireless LAN 802.11n USB 2.0 Network Adapter"
Compare-1.DeviceDesc.DispName		= "Compare Wireless LAN 802.11n USB 2.0 Network Adapter"
;*******************************************************************************
; RTL8723au Device description
;*******************************************************************************
RTL8723au.DeviceDesc 				= "Realtek RTL8723AU Wireless LAN 802.11n USB 2.0 Network Adapter"
RTL8723au.DeviceDesc.DispName		= "Realtek RTL8723AU Wireless LAN 802.11n USB 2.0 Network Adapter"
;*******************************************************************************
; RTL8192DU Device description
;*******************************************************************************
RTL8192du.DeviceDesc 				= "Realtek RTL8192DU Wireless LAN 802.11n USB 2.0 Network Adapter"
RTL8192du.DeviceDesc.DispName		        = "Realtek RTL8192DU Wireless LAN 802.11n USB 2.0 Network Adapter"
RTL8192du0.DeviceDesc 				= "Realtek RTL8192DU Wireless LAN 802.11n USB 2.0 Network Adapter MAC0"
RTL8192du0.DeviceDesc.DispName		        = "Realtek RTL8192DU Wireless LAN 802.11n USB 2.0 Network Adapter MAC0"
RTL8192du1.DeviceDesc 				= "Realtek RTL8192DU Wireless LAN 802.11n USB 2.0 Network Adapter MAC1"
RTL8192du1.DeviceDesc.DispName		        = "Realtek RTL8192DU Wireless LAN 802.11n USB 2.0 Network Adapter MAC1"
RTL8192du2.DeviceDesc           	= "Realtek RTL8192DU Wireless LAN 802.11N USB 2.0 Network Adapter MAC0"
RTL8192du2.DeviceDesc.DispName		= "Realtek RTL8192DU Wireless LAN 802.11n USB 2.0 Network Adapter MAC0"
RTL8192du3.DeviceDesc           	= "Realtek RTL8192DU Wireless LAN 802.11n USB 2.0 Network Adapter MAC1"
RTL8192du3.DeviceDesc.DispName		= "Realtek RTL8192DU Wireless LAN 802.11n USB 2.0 Network Adapter MAC1"
Belkin-N600DB.DeviceDesc		= "Belkin Wireless Adapter"
Belkin-N600DB.DeviceDesc.DispName	= "Belkin Wireless Adapter"
Belkin-N450DB.DeviceDesc		= "Belkin Wireless Adapter"
Belkin-N450DB.DeviceDesc.DispName	= "Belkin Wireless Adapter"
Belkin-N300DB.DeviceDesc		= "Belkin Wireless Adapter"
Belkin-N300DB.DeviceDesc.DispName	= "Belkin Wireless Adapter"
DLink-DWA151.DeviceDesc                 = "D-Link DWA-151 Wireless N 150 dual band USB Adapter"   
DLink-DWA151.DeviceDesc.DispName        = "D-Link DWA-151 Wireless N 150 dual band USB Adapter"  
;*******************************************************************************
; RTL8188EU Device description
;*******************************************************************************
RTL8188eu.DeviceDesc 				= "Realtek RTL8188EU Wireless LAN 802.11n USB 2.0 Network Adapter"
RTL8188eu.DeviceDesc.DispName		= "Realtek RTL8188EU Wireless LAN 802.11n USB 2.0 Network Adapter"
RTL8195au_os60.DeviceDesc 				= "Realtek RTL8195AU Wireless LAN 802.11ac USB 2.0 Network Adapter"
RTL8195au_os60.DeviceDesc.DispName		= "Realtek RTL8195AU Wireless LAN 802.11ac USB 2.0 Network Adapter"
RTL8195au.DeviceDesc 				= "Realtek RTL8195AU Wireless LAN 802.11ac USB 3.0 Network Adapter"
RTL8195au.DeviceDesc.DispName		= "Realtek RTL8195AU Wireless LAN 802.11ac USB 3.0 Network Adapter"