Home > Specifications > Interface Specifications

### Interface Specifications

USB *1 *2 | Hi-Speed USB 2.0 Use a USB 2.0 interface cable that is no longer than 6 feet (2 m).
LAN (For wired models) | 10BASE-T / 100BASE-TX Use a straight-through Category 5 (or greater) twisted-pair cable.
Wireless LAN (For models with wireless function) | IEEE 802.11b/g/n (Infrastructure/Ad-hoc Mode) IEEE 802.11g/n (Wi-Fi DirectTM)

*1
Your machine has a USB 2.0 Hi-Speed interface. The machine can also be connected to a computer that has a USB 1.1 interface.
*2
Third party USB ports are not supported.

Related Information
  - Specifications

Go to top of page